Dictionary

DocName

Project

Version

<< >>

FullName

UsedDocs

DocName Usage

Dictionary of keywords of the application domain

keyword reference description german actual user current user of a room Aktueller Benutzer actual value actual value Istwert

actuator device that can be controlled by control system or user Aktuator ambient light diffuse room lighting Umgebungslicht

blind used to shade window from the outside Jalousie ceiling light luminaire under or in the ceiling Deckenlicht

comfort temperature desired value of temperature during normal usage of a room Komforttemperatur

comfort time time period in which full room temperature comfort is expected Benutzungszeit

computer lab room with many terminals, workstations, open to all group members and temporarily to students of a class

Terminalraum

computer science department building building with typically offices, computer labs, peripheral rooms etc.

Informatikgebäude

contact electrical or magnetic gadget to determine the state of a door, window etc.

Kontakt

control panel small panel at the wall with a keyboard, LED’s for important states and a simple display for textual messages

Kontroll-Panel

control system hardware system and software system that controls indoor temperature and lighting

Kontrollsystem

customer persons, for whom the system is developed. Customers are always right.

Kunden

desired value variable entered, which the control system shall adjust and maintain.

Sollwert dimmer actuator controls the output of a luminaire Dimmer

door object which makes it possible to enter or leave a room Tür

environment surrounding of section of the building, indoor and outdoor Umgebung

facility manager person responsible for running a building on a daily bases Hausmeister

hallway part of a building between several rooms to connect each of them

Flur

heating period period of the year in which central heat is supplied Heizperiode heating up operation mode operation mode; the system tries to reach comfort temperature Aufheizmodus

heat-up time time in which comfort temperature is reached Aufheizzeit

hold temperature operation mode operation mode; the system tries to maintain the desired value of comfort temperature

Temperaturhaltemodus

illuminance amount of light incident on a surface, measured in lux Beleuchtungsstärke

impulse relais changes state ("on", "off") with each signal Stromstoßrelais

installation operative equipment belonging to the building, e.g. radiators and sensors

Installation

light scene light scenes are predefined settings of the light levels and an ordered list of luminaires which should be used to reach them. One light scene consists of 4 parameters:

1. name of light scene 2. illuminance of the ambient light of the room 3. illuminance for the desk 4. an ordered list, which consists the installed illuminaires. The order of the list is the order, in which the control system has to use the illuminaires to reach the given light values.

Lichtszene

light sensor measures the illuminance in a half sphere perpendicular to it’s flat bottom

Lichtsensor

luminaire light Licht motion detector imd detects motion of a person or animal in its range; state is "on" during positive detection

Bewegungsmelder

non freeze auto only non freeze safety should be maintained; typical operation mode during holidays

Frostschutzautomatikbetrieb

non freeze temperature value of temperature, which should not be reached to avoid freeze damage

Frostschutztemperatur

office room for one or two group members with terminals and/or workstations for inhabitants

Büro

off time time in which no usage is expected outdoor temperature temperature of the air outside Außentemperatur outdoor temperature sensor sensor to measure the temperature of the air outside Außentemperatursensor

peripheral room room for computer peripherals, copy machines, general group access

Peripherieraum

pushbutton "on", as long as pushed manually Taster radiator hot water radiator Heizkörper radiator control valve radiator valve that can be controlled Regelbares Heizkörperventil

radiator valve radiator valve that can be controlled manually Heizungsventil (manuell)

responsible person person responsible for individual settings of one room Verantwortliche Person

room room can be an office, meeting room, computer lab, or peripheral room.

Raum

room temperature temperature of the air in the room Raumtemperatur room temperature sensor sensor to measure the room temperature Raumtemperatursensor

sensor device that can sense state of the building, users or environment Sensor solar radiation Irradiance, measured in W/m^2 Sonneneinstrahlung

stand-by time time in which an inhabitant is expected in a room Stand-by-Zeit

status line a wire that has the status of a device as value switch sensor which gives "0" or "1" Schalter, als Sensor verwendet system system System task light luminaire on desk Arbeitsleuchte temperature sensor sensor, with whom the temperature can be measured Temperatursensor university building building in a university Universitätsgebäude user people inside the building Benutzer wait operation mode operation mode; the system waits until the user occupies a room for a longer time period.

Wartemodus

weather outdoor temperature, radiation Wetter window consists of a frame and glass, you can look through Fenster

Objects FullName ModelName ManufaktName Description

Attributes FullName ModelName Type Value Description

Signals FullName ModelName Type Link Parameters Description

Functions Name Task Strategy Needs